DOS Keyboard Scancodes
Listing of keyboard scancodes.
Description
Here follows a list of hardware keyboard scancodes accepted by the `MultiKey` function. These are equal to DOS scancodes, and are guaranteed to be always recognized on all platforms.
These constants are also defined in the `fbgfx.bi` include file you can use in your programs. If you are using the lang fb dialect then everything inside `fbgfx.bi` is enclosed in the `FB` `Namespace`. To use these constants in lang fb, either prepend "`FB.`" to the constant name, or put "`Using FB`" after the `#include` line.
The hexadecimal code is not required and provided only for reference.
`
SC_ESCAPE &h01
SC_1 &h02
SC_2 &h03
SC_3 &h04
SC_4 &h05
SC_5 &h06
SC_6 &h07
SC_7 &h08
SC_8 &h09
SC_9 &h0A
SC_0 &h0B
SC_MINUS &h0C
SC_EQUALS &h0D
SC_BACKSPACE &h0E
SC_TAB &h0F
SC_Q &h10
SC_W &h11
SC_E &h12
SC_R &h13
SC_T &h14
SC_Y &h15
SC_U &h16
SC_I &h17
SC_O &h18
SC_P &h19
SC_LEFTBRACKET &h1A
SC_RIGHTBRACKET &h1B
SC_ENTER &h1C
SC_CONTROL &h1D
SC_A &h1E
SC_S &h1F
SC_D &h20
SC_F &h21
SC_G &h22
SC_H &h23
SC_J &h24
SC_K &h25
SC_L &h26
SC_SEMICOLON &h27
SC_QUOTE &h28
SC_TILDE &h29
SC_LSHIFT &h2A
SC_BACKSLASH &h2B
SC_Z &h2C
SC_X &h2D
SC_C &h2E
SC_V &h2F
SC_B &h30
SC_N &h31
SC_M &h32
SC_COMMA &h33
SC_PERIOD &h34
SC_SLASH &h35
SC_RSHIFT &h36
SC_MULTIPLY &h37
SC_ALT &h38
SC_SPACE &h39
SC_CAPSLOCK &h3A
SC_F1 &h3B
SC_F2 &h3C
SC_F3 &h3D
SC_F4 &h3E
SC_F5 &h3F
SC_F6 &h40
SC_F7 &h41
SC_F8 &h42
SC_F9 &h43
SC_F10 &h44
SC_NUMLOCK &h45
SC_SCROLLLOCK &h46
SC_HOME &h47
SC_UP &h48
SC_PAGEUP &h49
SC_LEFT &h4B
SC_CLEAR &h4C
SC_CENTER &h4C
SC_RIGHT &h4D
SC_PLUS &h4E
SC_END &h4F
SC_DOWN &h50
SC_PAGEDOWN &h51
SC_INSERT &h52
SC_DELETE &h53
SC_F11 &h57
SC_F12 &h58
'' Extra scancodes not compatible with DOS scancodes
SC_LWIN &h5B
SC_RWIN &h5C
SC_MENU &h5D
`
See also

- `MultiKey`